**NAME**

**BLOCK**

**DATE**

**Directions:**

**Please answer the following questions by filling in the blanks as you watch the table saw safety video.**

1. **You should never wear ­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_ on your hands when operating a table saw.**
2. **Always use a ­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ when cutting stock that is 6” or less in width.**
3. **Never reach behind or over the blade until it \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ turning.**
4. **Never remove the \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ from a table saw – it is there for your protection.**
5. **Always inspect your \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ for hazards like knots and screws before you begin cutting.**
6. **Work should be release only when it is \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ the blade.**
7. **Always disconnect the \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ prior to changing the blade or performing maintenance on a table saw.**
8. **Always wear \_\_\_\_\_\_\_\_\_\_\_\_ glasses when using a table saw.**
9. **Never start the saw with the blade engaged with the \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.**
10. **Never attempt \_\_\_\_\_\_\_\_ hand cutting.**